                   .:                     :,                                          
,:::::::: ::`      :::                   :::                                          
,:::::::: ::`      :::                   :::                                          
.,,:::,,, ::`.:,   ... .. .:,     .:. ..`... ..`   ..   .:,    .. ::  .::,     .:,`   
   ,::    :::::::  ::, :::::::  `:::::::.,:: :::  ::: .::::::  ::::: ::::::  .::::::  
   ,::    :::::::: ::, :::::::: ::::::::.,:: :::  ::: :::,:::, ::::: ::::::, :::::::: 
   ,::    :::  ::: ::, :::  :::`::.  :::.,::  ::,`::`:::   ::: :::  `::,`   :::   ::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  :::::: ::::::::: ::`   :::::: ::::::::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  .::::: ::::::::: ::`    ::::::::::::::: 
   ,::    ::.  ::: ::, ::`  ::: ::: `:::.,::   ::::  :::`  ,,, ::`  .::  :::.::.  ,,, 
   ,::    ::.  ::: ::, ::`  ::: ::::::::.,::   ::::   :::::::` ::`   ::::::: :::::::. 
   ,::    ::.  ::: ::, ::`  :::  :::::::`,::    ::.    :::::`  ::`   ::::::   :::::.  
                                ::,  ,::                               ``             
                                ::::::::                                              
                                 ::::::                                               
                                  `,,`


https://www.thingiverse.com/thing:2667009
Carrot Cutter (Julienne) by shakethefuture is licensed under the Creative Commons - Attribution license.
http://creativecommons.org/licenses/by/3.0/

# Summary

Here we have a carrot cutter that will cut carrots in matchsticks with ease.
You’ll need a cheap caulk gun.
If you can’t find one locally, search for “Skeleton caulk gun” on Amazon.
Here is one similar to the one I used: https://goo.gl/FEKoRW
If you get the caulk gun mentioned above and it does not quite fit, let me know and I’ll make changes to the design.

Step 1:
Cut the end of the caulk gun

Step 2:
Apply some glue and slide the main 3D printed piece onto the caulk gun's side bars.

Step 3:
Use a steel wire to make a cutting end

Step 4:
Attach the plunger

Sep 5:
Pump the plunger until it reaches the cutter.

Step 6:
Cur the rod and glue the Lever.

Guide the carrot with a hand when you cut it.


# Check the video to see it in action

<iframe src="//www.youtube.com/embed/WnCOZATcKbU" frameborder="0" allowfullscreen></iframe>